Action htg=15, clg=26

+37.6076 if outdoor_temperature<=-4.5 & htg_setpoint<=20.0 & indoor_temperature<=21.1503 & HVAC_electricity_demand_rate>=1452.0250
+64.1777 if month<=2.0 & outdoor_temperature<=15.0 & htg_setpoint<=21.0 & indoor_temperature<=21.4391 & air_humidity<=62.4223
+32.9583 if outdoor_temperature<=8.8000 & clg_setpoint<=29.0 & 18.6568<=indoor_temperature<=20.6664 & air_humidity<=62.8327 & HVAC_electricity_demand_rate>=1782.9714
+26.2686 if hour<=6.0 & htg_setpoint<=20.0 & indoor_temperature<=19.9116 & air_humidity<=64.2343 & HVAC_electricity_demand_rate>=3492.0372
+21.9140 if outdoor_temperature<=-0.6000 & clg_setpoint>=24.0 & indoor_temperature<=19.7414 & air_humidity>=45.9442 & HVAC_electricity_demand_rate>=2194.6457
+16.8675 if month<=2.0 & day_of_month<=15.0 & 4.0<=hour<=11.0 & outdoor_temperature<=15.0 & clg_setpoint>=25.0 & 18.7904<=indoor_temperature<=21.4391 & air_humidity<=62.4223 & HVAC_electricity_demand_rate<=7581.2831
+13.5626 if outdoor_temperature<=1.1000 & 24.0<=clg_setpoint<=26.0 & indoor_temperature<=18.6655
+13.2045 if hour>=7.0 & outdoor_temperature<=-4.0 & clg_setpoint>=24.0 & indoor_temperature<=21.0219 & air_humidity<=62.2591 & HVAC_electricity_demand_rate<=6234.9341
+11.9701 if outdoor_temperature<=-1.2000 & clg_setpoint<=28.0 & indoor_temperature<=18.6297 & 20.1259<=air_humidity<=57.8947
+10.0043 if outdoor_temperature<=-9.5 & indoor_temperature<=21.3404 & air_humidity<=49.4593 & HVAC_electricity_demand_rate>=2895.6698
+9.1535 if day_of_month<=23.0 & hour>=22.0 & outdoor_temperature<=-0.6000 & htg_setpoint<=20.0 & clg_setpoint>=24.0 & indoor_temperature<=21.2843 & air_humidity>=22.2264 & HVAC_electricity_demand_rate<=10087.7751
+8.6395 if outdoor_temperature<=-1.2000 & htg_setpoint<=16.0 & indoor_temperature<=19.5284 & air_humidity>=45.6876

-------------------------------
Action htg=16, clg=26

+50.5500 if -11.7075<=outdoor_temperature<=15.0 & htg_setpoint<=20.0 & indoor_temperature<=20.8431
+42.3222 if hour<=6.0 & -9.5<=outdoor_temperature<=4.3200 & indoor_temperature<=21.1095
+33.7433 if hour<=6.0 & outdoor_temperature<=3.0 & HVAC_electricity_demand_rate>=3524.0383
+30.0530 if indoor_temperature<=19.4323 & HVAC_electricity_demand_rate>=3492.0372
+23.8401 if hour<=6.0 & outdoor_temperature<=-6.0 & HVAC_electricity_demand_rate>=1836.0156
+19.5165 if outdoor_temperature<=-5.0 & indoor_temperature<=20.8367 & air_humidity>=34.4557
+19.3194 if outdoor_temperature<=4.3200 & clg_setpoint<=26.0 & indoor_temperature<=20.7468 & air_humidity>=44.9061 & HVAC_electricity_demand_rate<=8328.7136
+17.1997 if outdoor_temperature<=-6.0 & indoor_temperature<=20.6569 & air_humidity>=34.4701
+12.2539 if outdoor_temperature<=1.1000 & indoor_temperature<=19.8760 & air_humidity>=48.4554 & HVAC_electricity_demand_rate>=2194.6457
+10.1033 if day_of_month<=16.0 & outdoor_temperature<=-9.5 & indoor_temperature<=21.4822
+9.9095 if outdoor_temperature<=-1.2000 & clg_setpoint<=28.0 & indoor_temperature<=18.6297 & 20.1259<=air_humidity<=57.8947
+6.5348 if hour<=5.0 & outdoor_temperature<=-6.2000 & air_humidity>=46.6687 & HVAC_electricity_demand_rate<=6047.4648

--------------------------------
Action htg=17, clg=26

+76.5049 if month<=2.0 & -9.5<=outdoor_temperature<=15.0 & htg_setpoint<=21.0 & indoor_temperature<=21.4391 & air_humidity<=58.7727
+43.0494 if -11.7075<=outdoor_temperature<=4.3200 & htg_setpoint>=17.0 & clg_setpoint<=26.0 & indoor_temperature<=21.2129 & HVAC_electricity_demand_rate>=1358.2302
+37.3332 if 4.0<=day_of_month<=25.0 & 10.0<=hour<=22.0 & clg_setpoint>=25.0 & indoor_temperature>=21.3982 & air_humidity<=53.3033 & HVAC_electricity_demand_rate>=1469.2592
+32.7592 if day_of_month<=28.0 & outdoor_temperature<=-2.0 & indoor_temperature<=20.5334 & air_humidity>=45.4178 & HVAC_electricity_demand_rate>=1428.0357
+25.5996 if -9.5<=outdoor_temperature<=-1.0 & htg_setpoint<=20.0 & indoor_temperature<=19.9116 & air_humidity<=58.9180 & HVAC_electricity_demand_rate>=3968.8338
+24.0059 if hour<=6.0 & -11.7075<=outdoor_temperature<=-3.4000 & htg_setpoint<=20.0 & clg_setpoint>=24.0 & indoor_temperature<=20.1179 & HVAC_electricity_demand_rate>=1291.2131
+23.3192 if hour<=7.0 & -9.5<=outdoor_temperature<=4.3200 & htg_setpoint>=18.0 & HVAC_electricity_demand_rate>=1543.1053
+21.3894 if 4.0<=day_of_month<=25.0 & hour>=12.0 & outdoor_temperature<=0.0 & indoor_temperature>=24.0490 & air_humidity<=53.7071 & 1423.5444<=HVAC_electricity_demand_rate<=3407.8832
+14.0182 if 2.0<=day_of_month<=27.0 & hour>=3.0 & -9.5<=outdoor_temperature<=-5.0 & htg_setpoint<=21.0 & indoor_temperature<=20.8367 & 28.6708<=air_humidity<=58.7727 & HVAC_electricity_demand_rate>=2252.5522
+11.4308 if hour<=6.0 & outdoor_temperature>=-9.5 & 46.0711<=air_humidity<=58.5575 & HVAC_electricity_demand_rate>=6373.5535
+8.6071 if -9.5<=outdoor_temperature<=-1.2000 & 20.4644<=indoor_temperature<=21.3840 & HVAC_electricity_demand_rate>=2085.9363
+7.9143 if day_of_month>=4.0 & 10.0<=hour<=16.0 & outdoor_temperature<=-4.5 & indoor_temperature>=21.4337 & air_humidity<=48.9116

--------------------------------
Action htg=18, clg=26

+52.4710 if outdoor_temperature<=2.0 & htg_setpoint>=18.0 & indoor_temperature>=24.6918 & 36.4788<=air_humidity<=59.9498 & 655.1863<=HVAC_electricity_demand_rate<=3286.0521
+31.8345 if -7.3000<=outdoor_temperature<=-2.4800 & clg_setpoint>=28.0 & indoor_temperature>=22.7824 & air_humidity<=53.0045 & HVAC_electricity_demand_rate<=2804.0908
+25.6196 if day_of_month<=23.0 & hour>=21.0 & htg_setpoint>=18.0 & indoor_temperature<=21.2843 & 22.2264<=air_humidity<=57.4836 & HVAC_electricity_demand_rate<=4727.3044
+14.6693 if hour<=16.0 & clg_setpoint>=28.0 & 24.3635<=indoor_temperature<=25.3421 & air_humidity<=43.6038 & 1974.6005<=HVAC_electricity_demand_rate<=2847.7105
+12.8951 if day_of_month>=17.0 & 1.0<=hour<=5.0 & htg_setpoint<=16.0 & indoor_temperature<=19.6280 & HVAC_electricity_demand_rate>=728.1273
+6.6281 if 14.0<=hour<=15.0 & outdoor_temperature<=-2.4800 & 24.1909<=indoor_temperature<=25.1225 & air_humidity<=44.0097 & HVAC_electricity_demand_rate<=2856.4850
+3.6962 if outdoor_temperature<=-2.4800 & indoor_temperature>=25.9993
+2.2511 if hour>=18.0 & -5.0<=outdoor_temperature<=-2.4800 & indoor_temperature>=22.3801 & air_humidity<=52.5242 & 1164.7935<=HVAC_electricity_demand_rate<=1443.5973
+1.7191 if -7.3000<=outdoor_temperature<=-3.0 & clg_setpoint>=30.0 & air_humidity<=52.1981 & 1411.8365<=HVAC_electricity_demand_rate<=2783.3056
+1.6791 if 5.0<=day_of_month<=28.0 & -3.4000<=outdoor_temperature<=6.6000 & 22.4682<=indoor_temperature<=23.2356 & HVAC_electricity_demand_rate<=1559.4128

--------------------------------
Action htg=20, clg=26

+67.4353 if day_of_month<=26.0 & hour<=5.0 & -3.0<=outdoor_temperature<=5.0175 & htg_setpoint<=21.0 & 24.0<=clg_setpoint<=29.0 & indoor_temperature<=20.4542 & air_humidity>=33.8024
+32.3240 if day_of_month<=25.0 & hour<=7.0 & outdoor_temperature<=-6.2000 & indoor_temperature<=19.3978 & air_humidity>=48.3545
+29.2159 if 2.0<=hour<=21.0 & outdoor_temperature<=-6.2000 & htg_setpoint=18.0 & indoor_temperature<=19.3432 & air_humidity<=58.7727
+28.7860 if day_of_month<=25.0 & hour<=16.0 & outdoor_temperature<=-5.0 & indoor_temperature>=22.4146
+16.0746 if outdoor_temperature<=-6.2000 & indoor_temperature>=23.2736 & 2628.6807<=HVAC_electricity_demand_rate<=4816.4221
+15.5775 if hour>=10.0 & outdoor_temperature<=-6.2000 & htg_setpoint>=18.0 & indoor_temperature>=22.2746 & air_humidity>=35.9678 & HVAC_electricity_demand_rate>=2914.4970
+15.5761 if hour<=15.0 & outdoor_temperature<=-6.0 & indoor_temperature>=23.0022
+14.0541 if hour<=16.0 & outdoor_temperature<=-5.0 & indoor_temperature>=23.5872 & HVAC_electricity_demand_rate<=3378.0424
+13.0024 if day_of_month<=4.0 & hour<=17.0 & outdoor_temperature<=-5.0 & indoor_temperature>=22.9998 & 32.5154<=air_humidity<=42.6080 & HVAC_electricity_demand_rate>=2841.4206
+11.6762 if outdoor_temperature<=-6.0 & htg_setpoint>=20.0 & air_humidity<=42.6534
+7.7685 if outdoor_temperature<=-9.5 & indoor_temperature>=23.2181 & air_humidity<=40.6845
+7.4560 if outdoor_temperature<=-7.3000 & indoor_temperature>=22.4197 & air_humidity<=40.2033

--------------------------------
Action htg=21, clg=26

-88.9567 if outdoor_temperature<=3.0 & htg_setpoint>=21.0 & indoor_temperature<=21.3094
-20.6252 if outdoor_temperature<=3.0 & clg_setpoint>=25.0 & indoor_temperature<=21.4071 & air_humidity<=31.0682 & HVAC_electricity_demand_rate>=2541.7048
-20.4274 if HVAC_electricity_demand_rate>=14049.8896
-19.6657 if day_of_month<=27.0 & hour>=6.0 & -11.7075<=outdoor_temperature<=-3.9000 & htg_setpoint<=18.0 & indoor_temperature<=19.9367 & air_humidity<=58.7727 & HVAC_electricity_demand_rate>=1899.6352
-16.1636 if outdoor_temperature<=-6.2000 & clg_setpoint<=24.0 & air_humidity>=45.8796 & HVAC_electricity_demand_rate>=5119.5404
-11.3369 if indoor_temperature<=20.7008 & HVAC_electricity_demand_rate>=14578.3255
-10.5239 if clg_setpoint>=29.0 & HVAC_electricity_demand_rate>=3067.5452
-7.3994 if day_of_month>=12.0 & 19.0<=hour<=21.0 & -4.0<=outdoor_temperature<=-3.9000 & air_humidity>=29.8473
-3.4527 if 6.0<=day_of_month<=30.0 & -4.5<=outdoor_temperature<=4.3200 & htg_setpoint>=16.0 & clg_setpoint<=28.0 & 22.9216<=indoor_temperature<=24.5265 & HVAC_electricity_demand_rate<=2827.9858
+8.1599 if outdoor_temperature<=-2.4800 & clg_setpoint<=23.0
+5.9809 if hour<=3.0 & outdoor_temperature>=15.0 & air_humidity>=61.9269
+3.2909 if day_of_month<=25.0 & outdoor_temperature>=-3.4000 & 23.0133<=indoor_temperature<=24.5817 & air_humidity<=38.6007 & 1543.1053<=HVAC_electricity_demand_rate<=2427.6149

--------------------------------
Action htg=22, clg=26

+43.3846 if month<=2.0 & -11.7075<=outdoor_temperature<=13.0150 & 15.0<=htg_setpoint<=21.0 & 18.1197<=indoor_temperature<=22.9990 & 18.1311<=air_humidity<=62.4223 & HVAC_electricity_demand_rate<=16869.0802
+43.0561 if outdoor_temperature<=5.0175 & indoor_temperature<=21.0199 & air_humidity<=63.3224
+42.8342 if month<=2.0 & outdoor_temperature<=13.0150 & htg_setpoint<=21.0 & clg_setpoint<=29.0 & indoor_temperature<=21.3982
+27.1310 if outdoor_temperature<=8.8000 & indoor_temperature<=20.6664 & HVAC_electricity_demand_rate>=2697.1032
+26.2469 if hour<=6.0 & outdoor_temperature<=7.2125 & htg_setpoint<=18.0 & indoor_temperature<=20.8405 & HVAC_electricity_demand_rate>=527.5443
+21.1123 if hour>=2.0 & outdoor_temperature<=-3.4000 & clg_setpoint>=24.0 & indoor_temperature<=20.2879 & air_humidity<=62.2591 & HVAC_electricity_demand_rate<=8781.6791
+20.7029 if 3.0<=day_of_month<=29.0 & hour<=11.0 & outdoor_temperature<=11.0 & clg_setpoint<=29.0 & 18.4192<=indoor_temperature<=20.0000 & 18.1311<=air_humidity<=62.4223 & HVAC_electricity_demand_rate<=8623.5397
+18.8706 if indoor_temperature<=18.7904 & HVAC_electricity_demand_rate>=1462.0127
+17.5153 if day_of_month>=5.0 & 1.0<=hour<=22.0 & outdoor_temperature<=0.0 & htg_setpoint>=16.0 & indoor_temperature<=19.6442 & air_humidity>=18.4414 & 1766.3143<=HVAC_electricity_demand_rate<=9086.7766
+17.4994 if hour<=6.0 & outdoor_temperature<=1.1000 & htg_setpoint<=18.0 & indoor_temperature<=19.7608 & HVAC_electricity_demand_rate>=3492.0372
+15.8718 if hour<=6.0 & indoor_temperature<=19.4393 & air_humidity>=43.0722 & HVAC_electricity_demand_rate>=628.5598
+15.4239 if hour<=6.0 & outdoor_temperature<=-6.0 & htg_setpoint<=20.0 & HVAC_electricity_demand_rate>=1836.0156

--------------------------------
Action htg=18, clg=23

+51.1149 if month<=2.0 & day_of_month<=29.0 & -5.6000<=outdoor_temperature<=15.0 & indoor_temperature<=22.1764 & air_humidity>=18.1311 & HVAC_electricity_demand_rate<=13459.1829
+28.1908 if day_of_month<=29.0 & -5.6000<=outdoor_temperature<=0.0 & htg_setpoint<=21.0 & clg_setpoint>=24.0 & indoor_temperature<=21.3745 & air_humidity>=18.4414
+26.1528 if 9.0<=day_of_month<=29.0 & hour>=3.0 & -2.0<=outdoor_temperature<=15.0 & clg_setpoint<=29.0 & indoor_temperature<=22.1764 & air_humidity>=18.1311 & HVAC_electricity_demand_rate<=13459.1829
+25.5588 if day_of_month<=28.0 & outdoor_temperature>=-5.6000 & indoor_temperature<=19.1094 & air_humidity>=19.3637 & HVAC_electricity_demand_rate>=628.2020
+21.2600 if month<=2.0 & -5.6000<=outdoor_temperature<=7.2125 & htg_setpoint>=15.0 & indoor_temperature<=20.7310 & air_humidity>=17.3376 & HVAC_electricity_demand_rate<=2595.9328
+16.5137 if day_of_month<=28.0 & -5.6000<=outdoor_temperature<=5.0175 & indoor_temperature<=20.2126 & HVAC_electricity_demand_rate>=3299.0534
+11.0762 if month<=2.0 & 0.5<=outdoor_temperature<=15.0 & clg_setpoint>=25.0 & indoor_temperature<=21.3840
+7.9097 if month<=2.0 & -1.2000<=outdoor_temperature<=15.0 & indoor_temperature<=21.5158 & HVAC_electricity_demand_rate<=875.5596
+5.2537 if hour>=4.0 & -5.6000<=outdoor_temperature<=1.1000 & indoor_temperature<=20.7008 & air_humidity>=62.2591 & HVAC_electricity_demand_rate>=944.2307
+4.5331 if air_humidity>=69.9883
+4.1963 if day_of_month>=3.0 & hour>=2.0 & -5.6000<=outdoor_temperature<=1.1000 & indoor_temperature<=19.8760 & air_humidity>=51.8004 & HVAC_electricity_demand_rate>=2194.6457
+2.9648 if day_of_month<=28.0 & hour>=1.0 & -5.6000<=outdoor_temperature<=-4.5 & clg_setpoint<=26.0 & 18.1020<=indoor_temperature<=21.5407 & 19.7914<=air_humidity<=59.6526

--------------------------------
Action htg=18, clg=24

+66.4324 if 3.0<=day_of_month<=27.0 & outdoor_temperature<=-6.0 & clg_setpoint<=29.0 & indoor_temperature<=23.1850 & air_humidity>=18.1311 & HVAC_electricity_demand_rate>=1899.6352
+40.4233 if 4.0<=day_of_month<=29.0 & hour>=18.0 & outdoor_temperature<=5.0175 & htg_setpoint<=21.0 & clg_setpoint>=24.0 & indoor_temperature<=21.4391 & HVAC_electricity_demand_rate>=719.0676
+38.7182 if day_of_month>=3.0 & outdoor_temperature<=-6.0 & indoor_temperature<=19.0323 & air_humidity>=46.7709
+26.1595 if hour<=6.0 & outdoor_temperature<=-6.2000 & clg_setpoint>=26.0 & indoor_temperature<=19.1278 & air_humidity>=46.7012
-26.6724 if day_of_month>=29.0 & indoor_temperature>=25.1097 & HVAC_electricity_demand_rate<=628.0451
+14.7757 if day_of_month>=3.0 & hour<=21.0 & outdoor_temperature<=-6.0 & 25.0<=clg_setpoint<=29.0 & air_humidity>=47.1406 & HVAC_electricity_demand_rate<=8190.0100
+14.3799 if day_of_month<=26.0 & -11.7075<=outdoor_temperature<=-6.0 & clg_setpoint<=24.0 & indoor_temperature<=19.4048 & air_humidity>=20.5012 & HVAC_electricity_demand_rate<=9833.1103
+12.1950 if 4.0<=day_of_month<=28.0 & hour>=22.0 & indoor_temperature<=20.7379 & air_humidity>=26.7369 & HVAC_electricity_demand_rate>=2690.0548
-12.8810 if clg_setpoint>=30.0 & indoor_temperature>=25.9988 & air_humidity>=60.7930
-10.8529 if outdoor_temperature<=-7.3000 & htg_setpoint>=20.0
+7.5359 if hour>=20.0 & HVAC_electricity_demand_rate>=8729.7106
+7.5359 if hour>=21.0 & HVAC_electricity_demand_rate>=8986.6480

--------------------------------
Action htg=18, clg=25

+76.0682 if month<=2.0 & day_of_month<=29.0 & -2.4800<=outdoor_temperature<=15.0 & htg_setpoint<=21.0 & indoor_temperature<=20.4542
+35.7797 if month<=2.0 & day_of_month<=28.0 & outdoor_temperature<=15.0 & indoor_temperature<=20.4547 & HVAC_electricity_demand_rate<=888.4346
+19.5429 if hour<=17.0 & outdoor_temperature<=4.3200 & indoor_temperature>=21.3982 & air_humidity>=22.1544 & HVAC_electricity_demand_rate>=3353.0663
+11.0059 if outdoor_temperature<=-7.3000 & indoor_temperature>=23.0022 & HVAC_electricity_demand_rate>=3343.0970
+10.4447 if month<=1.0 & outdoor_temperature<=0.0 & indoor_temperature>=22.3607 & air_humidity>=35.8469 & HVAC_electricity_demand_rate>=3237.7531
+9.2884 if day_of_month<=28.0 & -2.4800<=outdoor_temperature<=15.0 & clg_setpoint<=25.0 & indoor_temperature<=20.4644
+8.4585 if hour<=16.0 & indoor_temperature>=23.5872 & HVAC_electricity_demand_rate>=3378.0424
+7.6878 if 2.0<=day_of_month<=8.0 & hour<=15.0 & outdoor_temperature<=-6.7000 & indoor_temperature>=22.9565 & HVAC_electricity_demand_rate<=5120.2045
+6.0944 if hour<=16.0 & outdoor_temperature<=-9.5 & indoor_temperature>=22.3765
+6.0912 if -2.4800<=outdoor_temperature<=1.0 & clg_setpoint<=29.0 & indoor_temperature<=18.5048 & 28.1472<=air_humidity<=57.5569
+4.1747 if indoor_temperature>=25.1225 & HVAC_electricity_demand_rate>=4135.6304
+2.7032 if 2.0<=day_of_month<=29.0 & hour>=1.0 & -11.7075<=outdoor_temperature<=-5.6000 & 18.0977<=indoor_temperature<=24.9366 & 4026.8635<=HVAC_electricity_demand_rate<=7054.0210

--------------------------------
Action htg=18, clg=26

-36.2429 if month<=2.0 & hour<=21.0 & outdoor_temperature<=15.0 & indoor_temperature<=23.7285 & 30.4156<=air_humidity<=46.0647
+21.5354 if day_of_month<=29.0 & 1.0<=hour<=21.0 & outdoor_temperature<=3.0 & htg_setpoint<=18.0 & indoor_temperature<=19.3399 & 21.3773<=air_humidity<=42.7010 & HVAC_electricity_demand_rate>=3721.0240
-17.5853 if -4.5<=outdoor_temperature<=1.0 & 22.6279<=indoor_temperature<=23.7612 & 30.9608<=air_humidity<=45.2628
-12.9184 if 2.0<=hour<=20.0 & outdoor_temperature<=-8.4000 & 34.3280<=air_humidity<=43.6794 & HVAC_electricity_demand_rate>=2941.2918
-8.6023 if hour<=6.0 & outdoor_temperature<=0.5 & htg_setpoint<=18.0 & 29.6582<=air_humidity<=47.9879 & HVAC_electricity_demand_rate>=2963.7417
+8.0355 if hour<=21.0 & outdoor_temperature<=-7.3000 & htg_setpoint<=21.0 & 20.3061<=indoor_temperature<=23.7285 & air_humidity>=34.4557 & HVAC_electricity_demand_rate>=2895.1783
+6.9174 if day_of_month<=8.0 & hour<=22.0 & outdoor_temperature<=-9.5 & clg_setpoint>=26.0 & indoor_temperature<=19.0738 & air_humidity>=20.5696 & 6099.4350<=HVAC_electricity_demand_rate<=9405.0164
-5.1968 if hour<=21.0 & outdoor_temperature<=-8.4000 & indoor_temperature<=22.4683 & 33.3437<=air_humidity<=47.3246 & HVAC_electricity_demand_rate>=3013.0567
+4.6671 if outdoor_temperature<=-4.0 & 21.1003<=indoor_temperature<=23.6173 & 31.3661<=air_humidity<=46.2770
-4.3069 if day_of_month<=23.0 & 7.0<=hour<=11.0 & outdoor_temperature<=-5.0 & htg_setpoint>=18.0 & 18.0002<=indoor_temperature<=23.9983 & air_humidity>=30.9473
-4.2915 if hour<=21.0 & outdoor_temperature<=1.1000 & clg_setpoint<=26.0 & indoor_temperature<=18.7552 & 20.6283<=air_humidity<=44.9700 & 1859.3964<=HVAC_electricity_demand_rate<=6400.0092
-2.9940 if hour<=6.0 & htg_setpoint<=16.0 & air_humidity<=49.5334 & HVAC_electricity_demand_rate>=2255.9724

--------------------------------
Action htg=18, clg=28

+47.6207 if outdoor_temperature<=1.1000 & indoor_temperature<=21.3847
+42.5021 if month<=2.0 & outdoor_temperature<=13.0150 & clg_setpoint<=29.0 & indoor_temperature<=20.8932 & HVAC_electricity_demand_rate<=9236.5036
+37.5818 if month<=2.0 & htg_setpoint<=21.0 & 19.0381<=indoor_temperature<=22.2181 & air_humidity<=61.5915
+37.5560 if month<=2.0 & htg_setpoint<=21.0 & 19.0971<=indoor_temperature<=24.1215 & air_humidity<=62.4223
+26.1161 if outdoor_temperature<=-3.4000 & 17.0<=htg_setpoint<=18.0 & indoor_temperature<=21.6418 & HVAC_electricity_demand_rate>=1616.5198
+25.3651 if month<=2.0 & hour<=6.0 & outdoor_temperature<=8.8000 & indoor_temperature<=21.0920 & air_humidity<=51.7392
+21.4283 if hour<=6.0 & outdoor_temperature<=-2.0 & htg_setpoint<=18.0 & indoor_temperature<=20.0191 & HVAC_electricity_demand_rate>=1266.1656
+19.3831 if indoor_temperature<=19.0718
+18.9771 if clg_setpoint>=28.0 & indoor_temperature<=22.6279 & 3313.9887<=HVAC_electricity_demand_rate<=9094.2658
+15.9370 if outdoor_temperature<=1.0 & htg_setpoint<=20.0 & indoor_temperature<=21.1680 & air_humidity>=46.0692 & HVAC_electricity_demand_rate>=3766.4288
+11.4827 if outdoor_temperature<=1.1000 & indoor_temperature<=18.9835 & 2059.7858<=HVAC_electricity_demand_rate<=8526.6964
+11.1224 if 3.0<=day_of_month<=28.0 & hour>=22.0 & outdoor_temperature<=-1.0 & htg_setpoint<=18.0 & 20.5696<=air_humidity<=57.0262 & HVAC_electricity_demand_rate>=2007.6986

--------------------------------
Action htg=18, clg=29
-21.6942 if day_of_month<=17.0 & 1.0<=hour<=6.0 & outdoor_temperature<=-2.0 & htg_setpoint<=18.0 & 24.0<=clg_setpoint<=28.0 & indoor_temperature<=19.3432 & air_humidity<=49.5114
-20.8157 if day_of_month<=23.0 & hour<=20.0 & outdoor_temperature<=4.3200 & clg_setpoint<=29.0 & 21.3982<=indoor_temperature<=24.1856 & 28.9260<=air_humidity<=59.7814 & 1165.2383<=HVAC_electricity_demand_rate<=18283.5311
-18.9969 if day_of_month<=23.0 & hour<=20.0 & 21.5089<=indoor_temperature<=23.9646 & air_humidity>=28.2907 & HVAC_electricity_demand_rate>=1888.9573
-15.1487 if 5.0<=day_of_month<=24.0 & 4.0<=hour<=6.0 & outdoor_temperature<=-3.0 & clg_setpoint>=26.0 & indoor_temperature<=20.9084 & air_humidity>=22.2264 & HVAC_electricity_demand_rate>=4265.9727
-14.5951 if day_of_month<=23.0 & outdoor_temperature<=1.1000 & htg_setpoint>=16.0 & clg_setpoint<=29.0 & 22.8150<=indoor_temperature<=24.4758 & air_humidity>=29.8161 & 1423.5444<=HVAC_electricity_demand_rate<=3407.8832
-12.6463 if clg_setpoint>=29.0 & air_humidity<=24.5865 & HVAC_electricity_demand_rate>=7036.1158
-9.2568 if day_of_month>=3.0 & hour>=23.0 & outdoor_temperature<=1.0 & htg_setpoint<=18.0 & clg_setpoint>=25.0 & air_humidity>=28.3559 & HVAC_electricity_demand_rate<=4702.5667
-9.0428 if outdoor_temperature<=-4.0 & clg_setpoint>=28.0 & indoor_temperature<=24.8621 & air_humidity<=43.3357 & HVAC_electricity_demand_rate>=2485.6767
-6.2446 if day_of_month<=23.0 & outdoor_temperature<=0.5 & 23.9198<=indoor_temperature<=24.3778 & air_humidity>=32.2154 & HVAC_electricity_demand_rate>=1072.8742
-4.8127 if day_of_month<=23.0 & hour<=20.0 & outdoor_temperature<=-5.0 & clg_setpoint<=26.0 & 21.9479<=indoor_temperature<=24.4265 & air_humidity>=31.6533 & HVAC_electricity_demand_rate<=19214.6394
-3.6987 if day_of_month<=23.0 & hour<=20.0 & htg_setpoint>=22.0 & indoor_temperature>=21.6121 & 28.0282<=air_humidity<=59.5276 & HVAC_electricity_demand_rate>=2628.6807
+0.9638 if outdoor_temperature<=-2.48 & htg_setpoint<=16.0 & indoor_temperature>=23.2111

--------------------------------
Action htg=18, clg=30

+43.2454 if -7.3000<=outdoor_temperature<=1.1000 & htg_setpoint>=18.0 & indoor_temperature>=24.1098 & 30.1261<=air_humidity<=59.9072 & HVAC_electricity_demand_rate<=3545.0466
+27.2594 if day_of_month<=29.0 & -7.3000<=outdoor_temperature<=-1.2000 & 18.0<=htg_setpoint<=20.0 & indoor_temperature>=23.8952 & air_humidity<=59.4595 & HVAC_electricity_demand_rate<=3409.4454
+26.1286 if day_of_month>=4.0 & hour>=21.0 & htg_setpoint<=20.0 & clg_setpoint<=29.0 & 18.2009<=indoor_temperature<=20.9084 & air_humidity>=24.7034
+24.6603 if -7.3000<=outdoor_temperature<=1.1000 & htg_setpoint>=18.0 & indoor_temperature>=24.7505 & 36.6331<=air_humidity<=59.0649 & HVAC_electricity_demand_rate<=3417.4728
+16.0344 if -6.0<=outdoor_temperature<=-1.2000 & clg_setpoint>=29.0 & indoor_temperature>=23.6788 & air_humidity<=58.0867 & HVAC_electricity_demand_rate>=1046.7623
+12.5235 if hour<=16.0 & -7.3000<=outdoor_temperature<=-3.0 & indoor_temperature>=23.9984 & 32.9621<=air_humidity<=56.1589 & 1485.1843<=HVAC_electricity_demand_rate<=3534.1439
+11.3518 if day_of_month>=2.0 & hour<=16.0 & outdoor_temperature<=-2.4800 & htg_setpoint>=18.0 & indoor_temperature>=24.3635 & air_humidity<=44.6441 & HVAC_electricity_demand_rate<=3515.9828
+6.0009 if day_of_month>=4.0 & hour>=22.0 & outdoor_temperature<=-5.0 & htg_setpoint<=18.0 & indoor_temperature<=20.2656 & air_humidity>=44.6677
+5.2430 if outdoor_temperature<=-1.2000 & htg_setpoint=18.0 & indoor_temperature>=24.4489 & 1057.4154<=HVAC_electricity_demand_rate<=2621.9845
+5.0933 if day_of_month<=2.0 & outdoor_temperature<=-6.7000 & indoor_temperature>=24.1117
+4.9374 if day_of_month<=4.0 & outdoor_temperature<=-2.4800 & indoor_temperature>=24.2568 & air_humidity<=47.9028
+2.4272 if day_of_month>=7.0 & outdoor_temperature<=2.0 & htg_setpoint>=18.0 & indoor_temperature>=25.9991 & HVAC_electricity_demand_rate>=1588.5906

--------------------------------